R46 for OpenBVE ONLY - version 3.0.1
Train Programming & Sounds by error46146
Exterior View & Cab by Rikabs
Sign animations by CT1660
Additional help by Mr. Railfan
For more information visit www.bvestation.com

INSTRUCTIONS
Single handle train - 
use Z to add power/decrease brake;
use A to move to Neutral;
use Q to add brake/decrease power;
use 1 for Emergency Brake.
Full instructions can be found in the Information guide included with this train.

Extra controls - 
use 0 to control interior lighting
use 9 to control LCD sign lighting
use 8 to change LCD signs
use 7 to change Front Rollsigns
use 6 to activate/deactivate LAST STOP on LCD signs
use 5 to switch motormen

POWER POINTS
1 = Switching, 2 = Coast, 3 = Parallel
BRAKE POINTS
1 = Minimum, 5 = Full Service, EMG = Emergency

SPECIFICATIONS
Constructed 1975-1978, Refurbished 1990-1992
Unit Numbers: 5482 - 6258
Maximum Speed: 55mph
Length: 75ft
Motors: GE
Brakes: NYAB "SMEE" Brake System
Control: Cineston
Weight: 91,000lbs for cab cars, 86,670lbs for non-cab cars.
Source (for the above information): Wikipedia

If there are any questions or comments about the train, please contact the author at error46146@yahoo.com !

Thank you for downloading & Enjoy!